<?xml version="1.0"?>
<profile name="Tenlogy" version="2020-05-13 18:33:35" app="S3D-Software 4.1.2">
  <baseProfile>Default</baseProfile>
  <printMaterial>PLA</printMaterial>
  <printQuality>Medium</printQuality>
  <printExtruders>All Extruders</printExtruders>
  <extruder name="Extruder 1">
    <toolheadNumber>0</toolheadNumber>
    <diameter>0.4</diameter>
    <autoWidth>0</autoWidth>
    <width>0.45</width>
    <extrusionMultiplier>1</extrusionMultiplier>
    <useRetract>1</useRetract>
    <retractionDistance>1.5</retractionDistance>
    <extraRestartDistance>0</extraRestartDistance>
    <retractionZLift>0</retractionZLift>
    <retractionSpeed>2400</retractionSpeed>
    <useCoasting>0</useCoasting>
    <coastingDistance>0.2</coastingDistance>
    <useWipe>1</useWipe>
    <wipeDistance>3</wipeDistance>
  </extruder>
  <extruder name="Extruder 2">
    <toolheadNumber>1</toolheadNumber>
    <diameter>0.4</diameter>
    <autoWidth>0</autoWidth>
    <width>0.4</width>
    <extrusionMultiplier>0.96</extrusionMultiplier>
    <useRetract>1</useRetract>
    <retractionDistance>1.5</retractionDistance>
    <extraRestartDistance>0</extraRestartDistance>
    <retractionZLift>0</retractionZLift>
    <retractionSpeed>1800</retractionSpeed>
    <useCoasting>0</useCoasting>
    <coastingDistance>0.2</coastingDistance>
    <useWipe>1</useWipe>
    <wipeDistance>5</wipeDistance>
  </extruder>
  <primaryExtruder>0</primaryExtruder>
  <layerHeight>0.2</layerHeight>
  <topSolidLayers>6</topSolidLayers>
  <bottomSolidLayers>5</bottomSolidLayers>
  <perimeterOutlines>2</perimeterOutlines>
  <printPerimetersInsideOut>1</printPerimetersInsideOut>
  <startPointOption>2</startPointOption>
  <startPointOriginX>0</startPointOriginX>
  <startPointOriginY>0</startPointOriginY>
  <sequentialIslands>0</sequentialIslands>
  <spiralVaseMode>0</spiralVaseMode>
  <firstLayerHeightPercentage>100</firstLayerHeightPercentage>
  <firstLayerWidthPercentage>100</firstLayerWidthPercentage>
  <firstLayerUnderspeed>0.5</firstLayerUnderspeed>
  <useRaft>1</useRaft>
  <raftExtruder>1</raftExtruder>
  <raftTopLayers>2</raftTopLayers>
  <raftBaseLayers>1</raftBaseLayers>
  <raftOffset>3</raftOffset>
  <raftSeparationDistance>0</raftSeparationDistance>
  <raftTopInfill>100</raftTopInfill>
  <aboveRaftSpeedMultiplier>0.3</aboveRaftSpeedMultiplier>
  <useSkirt>1</useSkirt>
  <skirtExtruder>1</skirtExtruder>
  <skirtLayers>1</skirtLayers>
  <skirtOutlines>2</skirtOutlines>
  <skirtOffset>4</skirtOffset>
  <usePrimePillar>0</usePrimePillar>
  <primePillarExtruder>999</primePillarExtruder>
  <primePillarWidth>12</primePillarWidth>
  <primePillarLocation>7</primePillarLocation>
  <primePillarSpeedMultiplier>1</primePillarSpeedMultiplier>
  <useOozeShield>0</useOozeShield>
  <oozeShieldExtruder>999</oozeShieldExtruder>
  <oozeShieldOffset>2</oozeShieldOffset>
  <oozeShieldOutlines>1</oozeShieldOutlines>
  <oozeShieldSidewallShape>1</oozeShieldSidewallShape>
  <oozeShieldSidewallAngle>30</oozeShieldSidewallAngle>
  <oozeShieldSpeedMultiplier>1</oozeShieldSpeedMultiplier>
  <infillExtruder>0</infillExtruder>
  <internalInfillPattern>Grid</internalInfillPattern>
  <externalInfillPattern>Rectilinear</externalInfillPattern>
  <infillPercentage>25</infillPercentage>
  <outlineOverlapPercentage>15</outlineOverlapPercentage>
  <infillExtrusionWidthPercentage>100</infillExtrusionWidthPercentage>
  <minInfillLength>5</minInfillLength>
  <infillLayerInterval>1</infillLayerInterval>
  <internalInfillAngles>45,-45</internalInfillAngles>
  <overlapInternalInfillAngles>1</overlapInternalInfillAngles>
  <externalInfillAngles>45,-45</externalInfillAngles>
  <generateSupport>1</generateSupport>
  <supportExtruder>1</supportExtruder>
  <supportInfillPercentage>30</supportInfillPercentage>
  <supportExtraInflation>0.5</supportExtraInflation>
  <supportBaseLayers>1</supportBaseLayers>
  <denseSupportExtruder>1</denseSupportExtruder>
  <denseSupportLayers>2</denseSupportLayers>
  <denseSupportInfillPercentage>98</denseSupportInfillPercentage>
  <supportLayerInterval>1</supportLayerInterval>
  <supportHorizontalPartOffset>0.3</supportHorizontalPartOffset>
  <supportUpperSeparationLayers>0</supportUpperSeparationLayers>
  <supportLowerSeparationLayers>0</supportLowerSeparationLayers>
  <supportType>1</supportType>
  <supportGridSpacing>2</supportGridSpacing>
  <maxOverhangAngle>60</maxOverhangAngle>
  <supportAngles>0</supportAngles>
  <temperatureController name="Extruder 1">
    <temperatureNumber>0</temperatureNumber>
    <isHeatedBed>0</isHeatedBed>
    <stabilizeAtStartup>1</stabilizeAtStartup>
    <setpoint layer="1" temperature="215"/>
  </temperatureController>
  <temperatureController name="Extruder 2">
    <temperatureNumber>1</temperatureNumber>
    <isHeatedBed>0</isHeatedBed>
    <stabilizeAtStartup>1</stabilizeAtStartup>
    <setpoint layer="1" temperature="220"/>
  </temperatureController>
  <temperatureController name="Heated Bed">
    <temperatureNumber>0</temperatureNumber>
    <isHeatedBed>1</isHeatedBed>
    <stabilizeAtStartup>1</stabilizeAtStartup>
    <setpoint layer="1" temperature="60"/>
  </temperatureController>
  <fanSpeed>
    <setpoint layer="1" speed="0"/>
    <setpoint layer="2" speed="50"/>
    <setpoint layer="3" speed="100"/>
  </fanSpeed>
  <blipFanToFullPower>0</blipFanToFullPower>
  <adjustSpeedForCooling>1</adjustSpeedForCooling>
  <minSpeedLayerTime>15</minSpeedLayerTime>
  <minCoolingSpeedSlowdown>20</minCoolingSpeedSlowdown>
  <increaseFanForCooling>0</increaseFanForCooling>
  <minFanLayerTime>45</minFanLayerTime>
  <maxCoolingFanSpeed>100</maxCoolingFanSpeed>
  <increaseFanForBridging>0</increaseFanForBridging>
  <bridgingFanSpeed>100</bridgingFanSpeed>
  <use5D>1</use5D>
  <relativeEdistances>0</relativeEdistances>
  <allowEaxisZeroing>1</allowEaxisZeroing>
  <independentExtruderAxes>0</independentExtruderAxes>
  <includeM10123>0</includeM10123>
  <stickySupport>1</stickySupport>
  <applyToolheadOffsets>0</applyToolheadOffsets>
  <gcodeXoffset>0</gcodeXoffset>
  <gcodeYoffset>0</gcodeYoffset>
  <gcodeZoffset>0</gcodeZoffset>
  <overrideMachineDefinition>1</overrideMachineDefinition>
  <machineTypeOverride>0</machineTypeOverride>
  <strokeXoverride>305</strokeXoverride>
  <strokeYoverride>305</strokeYoverride>
  <strokeZoverride>360</strokeZoverride>
  <originOffsetXoverride>0</originOffsetXoverride>
  <originOffsetYoverride>0</originOffsetYoverride>
  <originOffsetZoverride>0</originOffsetZoverride>
  <homeXdirOverride>-1</homeXdirOverride>
  <homeYdirOverride>-1</homeYdirOverride>
  <homeZdirOverride>-1</homeZdirOverride>
  <flipXoverride>1</flipXoverride>
  <flipYoverride>-1</flipYoverride>
  <flipZoverride>1</flipZoverride>
  <toolheadOffsets>0,0|0,0|0,0|0,0|0,0|0,0</toolheadOffsets>
  <overrideFirmwareConfiguration>1</overrideFirmwareConfiguration>
  <firmwareTypeOverride>RepRap (Marlin/Repetier/Sprinter)</firmwareTypeOverride>
  <GPXconfigOverride>r2</GPXconfigOverride>
  <baudRateOverride>115200</baudRateOverride>
  <overridePrinterModels>0</overridePrinterModels>
  <printerModelsOverride></printerModelsOverride>
  <startingGcode>G21 ;metric values,G90 ;absolute positioning,M82 ;set extruder to absolute mode,M107 ;start with the fan off,G28 ;Move to min endstops,G1 Z0.5 F9000 ;move the platform down 0.5mm,,,,M117 Printing...</startingGcode>
  <layerChangeGcode></layerChangeGcode>
  <retractionGcode></retractionGcode>
  <toolChangeGcode>,,{IF NEWTOOL=1}T1,;switch to new tool and do these things,;{IF NEWTOOL=1}M109 S220 T1 ;heat right tool to 240C before moving,;{IF NEWTOOL=1}G1 F800 E-3.0,{IF NEWTOOL=1}G1 F800 E5.0 ;Default purge,{IF NEWTOOL=1}G4 S5 ;Stabilize Hotend's pressure dwell 5 seconds,{IF NEWTOOL=1}G92 E0 ;Zero extruder,{IF NEWTOOL=1}G1 F10000 X325,{IF NEWTOOL=1}G1 F2400 E-3 ;Retract,{IF NEWTOOL=1}G1 F10000 X354,{IF NEWTOOL=1}G1 F800 E-5 ;Retract,{IF NEWTOOL=1}G1 F10000,,,{IF NEWTOOL=0}T0,; switch to new tool and do these things,;{IF NEWTOOL=0}M104 S200 T1 ;let right extruder cool to 200 while unused,;{IF NEWTOOL=0}G1 F1200 E-2.0,{IF NEWTOOL=0}G1 F1000 E5.0 ;Default purge,{IF NEWTOOL=0}G4 S2 ;Stabilize Hotend's pressure with dwell for 2 seconds,{IF NEWTOOL=0}G92 E0 ;Zero extruder,{IF NEWTOOL=0}G1 F10000 X-20,{IF NEWTOOL=0}G1 F2400 E-3 ;Retract,{IF NEWTOOL=0}G1 F10000 X-50,{IF NEWTOOL=0}G1 F2400 E-5 ;Retract,{IF NEWTOOL=0}G1 F10000,</toolChangeGcode>
  <endingGcode>M104 T0 S0 ;1st extruder heater off,M104 T1 S0 ;2nd extruder heater off,M140 S0 ;heated bed heater off (if you have it),G91 ;relative positioning,G1 E-1 F300  ;retract the filament a bit before lifting the nozzle, to release some of the pressure,G1 Z+0.5 E-5 X-20 Y-20 F9000 ;move Z up a bit and retract filament even more,G28 X0 Y300 ;move X/Y to min endstops, so the head is out of the way,M84 ;steppers off,G90 ;absolute positioning</endingGcode>
  <exportFileFormat>gcode</exportFileFormat>
  <celebration>0</celebration>
  <celebrationSong>Random Song</celebrationSong>
  <postProcessing></postProcessing>
  <defaultSpeed>3600</defaultSpeed>
  <outlineUnderspeed>0.5</outlineUnderspeed>
  <solidInfillUnderspeed>0.8</solidInfillUnderspeed>
  <supportUnderspeed>0.8</supportUnderspeed>
  <rapidXYspeed>15000</rapidXYspeed>
  <rapidZspeed>1002</rapidZspeed>
  <minBridgingArea>50</minBridgingArea>
  <bridgingExtraInflation>0</bridgingExtraInflation>
  <bridgingExtrusionMultiplier>1</bridgingExtrusionMultiplier>
  <bridgingSpeedMultiplier>1</bridgingSpeedMultiplier>
  <useFixedBridgingAngle>0</useFixedBridgingAngle>
  <fixedBridgingAngle>0</fixedBridgingAngle>
  <applyBridgingToPerimeters>0</applyBridgingToPerimeters>
  <filamentDiameters>1.75|1.75|1.75|1.75|1.75|1.75</filamentDiameters>
  <filamentPricesPerKg>800|1500|46|46|46|46</filamentPricesPerKg>
  <filamentDensities>1|1|1.25|1.25|1.25|1.25</filamentDensities>
  <useMinPrintHeight>0</useMinPrintHeight>
  <minPrintHeight>0</minPrintHeight>
  <useMaxPrintHeight>0</useMaxPrintHeight>
  <maxPrintHeight>0</maxPrintHeight>
  <useDiaphragm>0</useDiaphragm>
  <diaphragmLayerInterval>20</diaphragmLayerInterval>
  <robustSlicing>1</robustSlicing>
  <mergeAllIntoSolid>0</mergeAllIntoSolid>
  <onlyRetractWhenCrossingOutline>0</onlyRetractWhenCrossingOutline>
  <retractBetweenLayers>1</retractBetweenLayers>
  <useRetractionMinTravel>0</useRetractionMinTravel>
  <retractionMinTravel>3</retractionMinTravel>
  <retractWhileWiping>1</retractWhileWiping>
  <onlyWipeOutlines>0</onlyWipeOutlines>
  <avoidCrossingOutline>0</avoidCrossingOutline>
  <maxMovementDetourFactor>3</maxMovementDetourFactor>
  <toolChangeRetractionDistance>3</toolChangeRetractionDistance>
  <toolChangeExtraRestartDistance>0</toolChangeExtraRestartDistance>
  <toolChangeRetractionSpeed>2400</toolChangeRetractionSpeed>
  <externalThinWallType>1</externalThinWallType>
  <internalThinWallType>1</internalThinWallType>
  <thinWallAllowedOverlapPercentage>50</thinWallAllowedOverlapPercentage>
  <singleExtrusionMinLength>1</singleExtrusionMinLength>
  <singleExtrusionMinPrintingWidthPercentage>50</singleExtrusionMinPrintingWidthPercentage>
  <singleExtrusionMaxPrintingWidthPercentage>200</singleExtrusionMaxPrintingWidthPercentage>
  <singleExtrusionEndpointExtension>0.2</singleExtrusionEndpointExtension>
  <horizontalSizeCompensation>0</horizontalSizeCompensation>
  <autoConfigureMaterial name="PLA">
    <temperatureController name="Extruder 1">
      <temperatureNumber>0</temperatureNumber>
      <isHeatedBed>0</isHeatedBed>
      <stabilizeAtStartup>1</stabilizeAtStartup>
      <setpoint layer="1" temperature="215"/>
    </temperatureController>
    <temperatureController name="Extruder 2">
      <temperatureNumber>1</temperatureNumber>
      <isHeatedBed>0</isHeatedBed>
      <stabilizeAtStartup>1</stabilizeAtStartup>
      <setpoint layer="1" temperature="220"/>
    </temperatureController>
    <globalBedTemperature>60</globalBedTemperature>
    <extruder name="Extruder 1">
      <toolheadNumber>0</toolheadNumber>
      <diameter>0.4</diameter>
      <autoWidth>0</autoWidth>
      <width>0.45</width>
      <extrusionMultiplier>1</extrusionMultiplier>
      <useRetract>1</useRetract>
      <retractionDistance>1.5</retractionDistance>
      <extraRestartDistance>0</extraRestartDistance>
      <retractionZLift>0</retractionZLift>
      <retractionSpeed>2400</retractionSpeed>
      <useCoasting>0</useCoasting>
      <coastingDistance>0.2</coastingDistance>
      <useWipe>1</useWipe>
      <wipeDistance>3</wipeDistance>
    </extruder>
    <extruder name="Extruder 2">
      <toolheadNumber>1</toolheadNumber>
      <diameter>0.4</diameter>
      <autoWidth>0</autoWidth>
      <width>0.4</width>
      <extrusionMultiplier>0.96</extrusionMultiplier>
      <useRetract>1</useRetract>
      <retractionDistance>1.5</retractionDistance>
      <extraRestartDistance>0</extraRestartDistance>
      <retractionZLift>0</retractionZLift>
      <retractionSpeed>1800</retractionSpeed>
      <useCoasting>0</useCoasting>
      <coastingDistance>0.2</coastingDistance>
      <useWipe>1</useWipe>
      <wipeDistance>5</wipeDistance>
    </extruder>
    <fanSpeed>
      <setpoint layer="1" speed="0"/>
      <setpoint layer="2" speed="50"/>
      <setpoint layer="3" speed="100"/>
    </fanSpeed>
  </autoConfigureMaterial>
  <autoConfigureMaterial name="ABS">
    <globalExtruderTemperature>225</globalExtruderTemperature>
    <globalBedTemperature>100</globalBedTemperature>
    <globalExtrusionMultiplier>1</globalExtrusionMultiplier>
    <fanSpeed>
      <setpoint layer="1" speed="0"/>
    </fanSpeed>
  </autoConfigureMaterial>
  <autoConfigureMaterial name="PVA">
    <globalExtruderTemperature>195</globalExtruderTemperature>
    <globalBedTemperature>80</globalBedTemperature>
    <globalExtrusionMultiplier>1</globalExtrusionMultiplier>
    <fanSpeed>
      <setpoint layer="1" speed="0"/>
      <setpoint layer="2" speed="100"/>
    </fanSpeed>
  </autoConfigureMaterial>
  <autoConfigureMaterial name="Nylon">
    <globalExtruderTemperature>220</globalExtruderTemperature>
    <globalBedTemperature>80</globalBedTemperature>
    <globalExtrusionMultiplier>1</globalExtrusionMultiplier>
    <fanSpeed>
      <setpoint layer="1" speed="0"/>
    </fanSpeed>
  </autoConfigureMaterial>
  <autoConfigureQuality name="Fast">
    <layerHeight>0.3</layerHeight>
    <topSolidLayers>3</topSolidLayers>
    <bottomSolidLayers>3</bottomSolidLayers>
    <skirtLayers>1</skirtLayers>
    <infillPercentage>15</infillPercentage>
    <supportInfillPercentage>25</supportInfillPercentage>
  </autoConfigureQuality>
  <autoConfigureQuality name="Medium">
    <layerHeight>0.2</layerHeight>
    <topSolidLayers>6</topSolidLayers>
    <bottomSolidLayers>5</bottomSolidLayers>
    <skirtLayers>1</skirtLayers>
    <infillPercentage>25</infillPercentage>
    <supportInfillPercentage>30</supportInfillPercentage>
  </autoConfigureQuality>
  <autoConfigureQuality name="High">
    <layerHeight>0.1</layerHeight>
    <topSolidLayers>4</topSolidLayers>
    <bottomSolidLayers>4</bottomSolidLayers>
    <skirtLayers>2</skirtLayers>
    <infillPercentage>30</infillPercentage>
    <supportInfillPercentage>40</supportInfillPercentage>
  </autoConfigureQuality>
  <autoConfigureExtruders name="Extruder 1 Only" allowedToolheads="1">
    <primaryExtruder>0</primaryExtruder>
    <raftExtruder>0</raftExtruder>
    <skirtExtruder>0</skirtExtruder>
    <infillExtruder>0</infillExtruder>
    <supportExtruder>1</supportExtruder>
    <denseSupportExtruder>1</denseSupportExtruder>
    <useSkirt>1</useSkirt>
    <usePrimePillar>0</usePrimePillar>
    <useOozeShield>0</useOozeShield>
    <startingGcode>G21 ;metric values,G90 ;absolute positioning,M82 ;set extruder to absolute mode,M107 ;start with the fan off,G28 ;Move to min endstops,G1 Z15.0 F9000 ;move the platform down 15mm,G1 X0.1 Y20 Z0.3 F5000.0 ; move to start-line position,G1 X0.1 Y200.0 Z0.3 F1500.0 E15 ; draw 1st line,G1 X0.4 Y200.0 Z0.3 F5000.0 ; move to side a little,G1 X0.4 Y20 Z0.3 F1500.0 E30 ; draw 2nd line,; G1 E27 F3000 ; retract filament 3mm,G92 E0 ; reset extruder,; done purging extruder,G1 Z1.0 F3000 ; move z up little to prevent scratching of surface,M117 Printing...</startingGcode>
    <toggleTemperatureController name="Extruder 1" status="on" stabilize="on"/>
    <toggleTemperatureController name="Extruder 2" status="on" stabilize="off"/>
  </autoConfigureExtruders>
  <autoConfigureExtruders name="Extruder 2 Only" allowedToolheads="1">
    <primaryExtruder>1</primaryExtruder>
    <raftExtruder>1</raftExtruder>
    <skirtExtruder>1</skirtExtruder>
    <infillExtruder>1</infillExtruder>
    <supportExtruder>1</supportExtruder>
    <denseSupportExtruder>1</denseSupportExtruder>
    <useSkirt>1</useSkirt>
    <usePrimePillar>0</usePrimePillar>
    <useOozeShield>0</useOozeShield>
    <startingGcode>G28 ; home all axes</startingGcode>
    <toggleTemperatureController name="Extruder 1" status="off" stabilize="off"/>
    <toggleTemperatureController name="Extruder 2" status="on" stabilize="on"/>
  </autoConfigureExtruders>
  <autoConfigureExtruders name="All Extruders" allowedToolheads="2">
    <primaryExtruder>0</primaryExtruder>
    <raftExtruder>1</raftExtruder>
    <skirtExtruder>1</skirtExtruder>
    <infillExtruder>0</infillExtruder>
    <supportExtruder>1</supportExtruder>
    <denseSupportExtruder>1</denseSupportExtruder>
    <useSkirt>1</useSkirt>
    <usePrimePillar>0</usePrimePillar>
    <useOozeShield>0</useOozeShield>
    <startingGcode>G21 ;metric values,G90 ;absolute positioning,M82 ;set extruder to absolute mode,M107 ;start with the fan off,G28 ;Move to min endstops,G1 Z0.5 F9000 ;move the platform down 0.5mm,,,,M117 Printing...</startingGcode>
    <toggleTemperatureController name="Extruder 1" status="on" stabilize="on"/>
    <toggleTemperatureController name="Extruder 2" status="on" stabilize="on"/>
  </autoConfigureExtruders>
</profile>
